**STEINEL Professional Presence detector**

**IR Quattro HD**

**LiveLink**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 50 mm; Number of DALI users: 3; Sensor Technology: passive infrared; Application, place: Indoors; Application, place, room: Open-plan office, high-bay warehouse, conference room, sports hall, classroom; Installation site: ceiling; Type of installation: Concealed wiring; Switching zones: 4800 switching zones; Electronic scalability: No; Mechanical scalability: Yes; Mounting height: 2,50 – 10,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Reach, radial: 8 x 8 m (64 m²); Reach, tangential: 20 x 20 m (400 m²); Reach, presence: 8 x 8 m (64 m²); Twilight setting TEACH: Yes; Time setting: 30 sec – 60 min; LiveLink values: Light level, Motion detection; With bus coupling: Yes; Settings via: LiveLink app; With remote control: No; IP rating: IP20; Material: Plastic; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: LiveLink; PU1, EAN: 4007841009717

**Manufacturer** Steinel

**Prod. No.** 009717

**Ordering designation** IR Quattro HD LiveLink

Deliver, install and set ready for operation