**STEINEL Professional Presence detector**

**HF 360**

**DALI**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 56 mm; Mains power supply: 230 V, 50 / 60 Hz; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: side room, stairwell, washroom, wc; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Control output, DALI: Broadcast 2x12 electronic ballasts; Constant-lighting control: Yes; Basic light level function: Yes; Basic light level function in per cent: 10 – 60 %; Basic light level function time: 1-60 min, all night; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 60 %; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: DALI; PU1, EAN: 4007841002817

**Manufacturer** Steinel

**Prod. No.** 002817

**Ordering designation** HF 360 DALI

Deliver, install and set ready for operation