**STEINEL Professional Presence detector**

**HF 360**

**DALI-2**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 56 mm; Mains power supply: 12 – 22,5 V; Power supply, detail: DALI bus; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: side room, stairwell, washroom, wc; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Twilight setting: 10 – 1000 lx; Switching output 1, floating: No; Switching output 2, floating: No; Control output, DALI: Addressable/slave; With remote control: No; Interconnection: Yes; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: DALI-2; PU1, EAN: 4007841057480

**Manufacturer** Steinel

**Prod. No.** 057480

**Ordering designation** HF 360 DALI2

Deliver, install and set ready for operation