**STEINEL Professional Presence detector**

**HF 360**

**V2 KNX**

Type: Presence detector; Dimensions (L x W x H): 56 x 120 x 120 mm; Power supply, detail: KNX bus; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: side room, stairwell, washroom, wc; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 0 – 255 min; Basic light level function in per cent: 10 – 50 %; Basic light level function time: Permanently ON, 1-255 min, all night; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 50 %; KNX functions: Light output 4x, Presence output, Light level, Constant-lighting control, Basic light level function, HVAC output; With bus coupling: Yes; Settings via: ETS software, Remote control, Bus; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: KNX; PU1, EAN: 4007841008796

**Manufacturer** Steinel

**Prod. No.** 008796

**Ordering designation** HF 360 KNX V2

Deliver, install and set ready for operation