**STEINEL Professional Presence detector**

**HF 360**

**LiveLink**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 36 mm; Power supply, detail: DALI bus; Number of DALI users: 4; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: side room, stairwell, washroom, wc; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Reach, detail: 1 or 2 detection directions can be masked out by stickers for adjustment to the room situation.; Reach, radial: Ø 12 m (113 m²); Reach, tangential: Ø 12 m (113 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 60 sec – 60 min; LiveLink values: Light level, Motion detection, Presence detection; With bus coupling: Yes; Settings via: LiveLink app; IP rating: IP20; Material: Plastic; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: LiveLink; PU1, EAN: 4007841033972

**Manufacturer** Steinel

**Prod. No.** 033972

**Ordering designation** HF 360 LiveLink

Deliver, install and set ready for operation