**STEINEL Professional Presence detector**

**US 360**

**COM1**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 68 mm; Mains power supply: 230 V, 50 / 60 Hz; Sensor Technology: Ultrasonic; Application, place: Indoors; Application, place, room: classroom, One-person office, Open-plan office, conference room, side room, stairwell, washroom, wc, equipment room; Installation site: ceiling; Type of installation: Concealed wiring; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Sneak-by guard: Yes; Reach, radial: Ø 10 m (79 m²); Reach, tangential: Ø 10 m (79 m²); Reach, presence: Ø 6 m (28 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Constant-lighting control: No; Basic light level function: No; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave, Master/master; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: COM1; PU1, EAN: 4007841007935

**Manufacturer** Steinel

**Prod. No.** 007935

**Ordering designation** US 360 COM1

Deliver, install and set ready for operation