**STEINEL Professional Presence detector**

**Dual US**

**V2 KNX**

Type: Presence detector; Dimensions (L x W x H): 73 x 120 x 120 mm; Power supply, detail: KNX bus; Sensor Technology: Ultrasonic; Application, place: Indoors; Application, place, room: corridor, aisle; Installation site: ceiling; Type of installation: Concealed wiring; Ultrasonic technology: 40 kHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Reach, radial: 20 x 3 m (60 m²); Reach, tangential: 20 x 3 m (60 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 60 sec – 255 min; KNX functions: Light output 4x, Presence output, Light level, Constant-lighting control, Basic light level function, HVAC output; With bus coupling: Yes; Settings via: ETS software, Remote control, Bus; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: KNX; PU1, EAN: 4007841029470

**Manufacturer** Steinel

**Prod. No.** 029470

**Ordering designation** DUAL US KNX

Deliver, install and set ready for operation