**STEINEL Professional Presence detector**

**Dual HF**

**COM1**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 75 mm; Mains power supply: 230 V, 50 / 60 Hz; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: corridor, aisle; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Reach, radial: 20 x 3 m (60 m²); Reach, tangential: 20 x 3 m (60 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Constant-lighting control: No; Basic light level function: No; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave, Master/master; IP rating: IP20; Material: Plastic; Ambient temperature: -25 – 50 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: COM1; PU1, EAN: 4007841002978

**Manufacturer** Steinel

**Prod. No.** 002978

**Ordering designation** DUAL HF COM1

Deliver, install and set ready for operation