**STEINEL Professional Presence detector**

**Dual HF**

**LiveLink**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 55 mm; Mains power supply: 230 V, 50 / 60 Hz; Number of DALI users: 8; Sensor Technology: High frequency; Application, place: Indoors; Application, place, room: corridor, aisle; Installation site: ceiling; Type of installation: Concealed wiring; HF-system: 5,8 GHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 140 °; Sneak-by guard: Yes; Reach, radial: 20 x 3 m (60 m²); Reach, tangential: 20 x 3 m (60 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 60 min; LiveLink values: Light level, Motion detection; Constant-lighting control: No; Basic light level function: No; With bus coupling: Yes; Settings via: LiveLink app; With remote control: No; Material: Plastic; Ambient temperature: -25 – 50 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: LiveLink; PU1, EAN: 4007841009700

**Manufacturer** Steinel

**Prod. No.** 009700

**Ordering designation** DUAL HF LiveLink

Deliver, install and set ready for operation