**STEINEL Professional Presence detector**

**IR Quattro MICRO**

**KNX**

Type: Presence detector; Dimensions (Ø x H): 43 x 70 mm; Mains power supply: 30 V; Power consumption: 0,5 W; Sensor Technology: passive infrared; Application, place: Indoors; Application, place, room: One-person office, side room, wc, washroom; Installation site: ceiling; Type of installation: Installation; Switching zones: 168 switching zones; Electronic scalability: No; Mechanical scalability: No; Mounting height: 2,00 – 5,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Time setting: 60 sec – 255 min; Constant-lighting control: Yes; Basic light level function: Yes; KNX functions: HVAC output, Basic light level function, Constant-lighting control, Light output 4x, Presence output, Light level; With bus coupling: Yes; With remote control: No; Interconnection: Yes; IP rating: IP65; Material: Plastic; Ambient temperature: -25 – 55 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: KNX; PU1, EAN: 4007841053864

**Manufacturer** Steinel

**Prod. No.** 053864

**Ordering designation** IR Quattro MICRO KNX

Deliver, install and set ready for operation