**STEINEL Professional Presence detector**

**IR Quattro SLIM XS**

**COM1 - square**

Type: Presence detector; Dimensions (L x W x H): 80 x 80 x 55 mm; Mains power supply: 220 – 240 V , 50 / 60 Hz; Sensor Technology: passive infrared; Application, place: Indoors; Application, place, room: classroom, One-person office, side room; Installation site: ceiling; Type of installation: Concealed wiring; Switching zones: 408 switching zones; Electronic scalability: No; Mechanical scalability: No; Mounting height: 2,50 – 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Reach, detail: Retina lens and hexagonal Fresnel structure; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 4 x 4 m (16 m²); Reach, presence: 4 x 4 m (16 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 30 sec – 30 min; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Constant-lighting control: No; Basic light level function: Yes; With remote control: Yes; Interconnection: Yes; Type of interconnection: Master/slave, Master/master; IP rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: COM1 - square; PU1, EAN: 4007841032951

**Manufacturer** Steinel

**Prod. No.** 032951

**Ordering designation** IR Quattro SLIM XS-Eckig COM1

Deliver, install and set ready for operation