**STEINEL Professional Presence detector**

**Single US**

**DALI-2**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 73 mm; Mains power supply: 16 V; Sensor Technology: Ultrasonic; Application, place: Indoors; Application, place, room: corridor, aisle, stairwell; Installation site: ceiling; Type of installation: Concealed wiring; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Detection angle: 180 °; Sneak-by guard: Yes; Reach, radial: 10 x 3 m (30 m²); Reach, tangential: 10 x 3 m (30 m²); Twilight setting: 10 – 1000 lx; Control output, DALI: Addressable/slave; With bus coupling: Yes; Interconnection: Yes; Material: Plastic; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: DALI-2; PU1, EAN: 4007841057503

**Manufacturer** Steinel

**Prod. No.** 057503

**Ordering designation** Single US DALI2

Deliver, install and set ready for operation