**STEINEL Professional Presence detector**

**Single US**

**LiveLink**

Type: Presence detector; Dimensions (L x W x H): 120 x 120 x 73 mm; Power supply, detail: DALI bus; Number of DALI users: 8; Sensor Technology: Ultrasonic; Application, place: Indoors; Application, place, room: corridor, aisle, stairwell; Installation site: ceiling; Type of installation: Concealed wiring; Ultrasonic technology: 40 kHz; Electronic scalability: Yes; Mechanical scalability: No; Mounting height: 2,50 – 3,50 m; Optimum mounting height: 2,8 m; Detection angle: 180 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Reach, radial: 10 x 3 m (30 m²); Reach, tangential: 10 x 3 m (30 m²); Twilight setting TEACH: Yes; Twilight setting: 10 – 1000 lx; Time setting: 60 sec – 60 min; LiveLink values: Light level, Motion detection; With bus coupling: Yes; Settings via: LiveLink app; Interconnection: Yes; IP rating: IP20; Material: Plastic; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: LiveLink; PU1, EAN: 4007841008437

**Manufacturer** Steinel

**Prod. No.** 008437

**Ordering designation** SINGLE US LiveLink

Deliver, install and set ready for operation